# List of actions

On the boot the device will load the default configuration that is programmed into the device.

In this default, the following instructions are made:

* Including the m32def.inc documentation
* Defining variables in the registers
* Declaring the origins for the interrupts and resets.

Afterwards when this is completed the program will run.

First off the program will go to the **init** label for initiating the Kristal timer.

Afterwards the program will go to the **loop** label

The program is waiting for the users input to set the time.